|  |
| --- |
|  |
|  |  |
| **TH-M6 Temperature Controllers 24 - 48 zones** |
| **GENERAL FEATURES*** Synchronous increase of temperatures
* “Slave” function: each zone can be linked to another with similar thermal behaviour
* Plastic leakage alarm
* Collective modification of all zones
* Immediate and complete diagnostic
* Efficient soft start (phase modulation adjustment)
* Elimination of absorption peaks on three-phase
* 2 independent set points
* Multi language
* Max working temperature: 50°C
* Main protection with circuit breaker
* 3-phase 400V supply or 3-phase 240V
* CE Certification
 | **TECHNICAL CHARACTERISTICS*** 16 A for each zone (3500 W) even simultaneously, thanks to the high heat exchange self ventilated heat sink
* Powerful control software:
	+ Recipes
	+ TEST environment to automatically test the electric connections of the heaters and of the temperature probes
	+ Process data and alarms log, graphic display and export
	+ Synoptic ambient with drag&drop function
	+ Log of executed operations
	+ "Undo" function
* High performing operator terminal:
	+ 10" LCD/TFT display
	+ 1024x600 (max 1024x768) resolution
	+ Aluminium front panel
	+ Touch screen

OPTIONAL* + Local or remote monitoring through Wi-fi or Ethernet connection
 |