|  |  |
| --- | --- |
| **TH-M6 Temperature Controllers up to 6-12 zone** | |
|  |  |
| **GENERAL FEATURES**   * Synchronous increase of temperatures * “Slave” function: each zone can be linked to  another with similar thermal behaviour * Plastic leakage alarm * Collective modification of all zones * Immediate and complete diagnostic * Efficient soft start (phase modulation adjustment) * Elimination of absorption peaks on three-phase * 2 independent set points * Multi language * Max working temperature: 50°C * Main protection with circuit breaker * 3-phase 400V supply or 3-phase 240V * CE Certification | **TECHNICAL CHARACTERISTICS**   * 16 A for each zone (3500 W) even simultaneously * Immediate and complete diagnostic * Wide graphic display 260x64 pixel * Scrolling messages help the operator in case of alarm * Dimensions 6 zones: 340 W x 160 H x 420 D mm * Dimensions 12 zones: 390 W x 210 H x 480 D mm   OPTIONAL   * Remote connection through serial RS485 interface * Support trolley up to 3 control units |