|  |
| --- |
| **TH-M6 Temperature Controllers up to 6-12 zone** |
|  |  |
| **GENERAL FEATURES*** Synchronous increase of temperatures
* “Slave” function: each zone can be linked to another with similar thermal behaviour
* Plastic leakage alarm
* Collective modification of all zones
* Immediate and complete diagnostic
* Efficient soft start (phase modulation adjustment)
* Elimination of absorption peaks on three-phase
* 2 independent set points
* Multi language
* Max working temperature: 50°C
* Main protection with circuit breaker
* 3-phase 400V supply or 3-phase 240V
* CE Certification
 | **TECHNICAL CHARACTERISTICS*** 16 A for each zone (3500 W) even simultaneously
* Immediate and complete diagnostic
* Wide graphic display 260x64 pixel
* Scrolling messages help the operator in case of alarm
* Dimensions 6 zones: 340 W x 160 H x 420 D mm
* Dimensions 12 zones: 390 W x 210 H x 480 D mm

OPTIONAL* Remote connection through serial RS485 interface
* Support trolley up to 3 control units
 |